(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Gyroscope & Accéléromètre")
		(date "06/06/2025")
		(company "UCAO-TECH")
		(comment 1 "Circuit électronique du test1 input")
		(comment 2 "TRC-2025")
	)
	(lib_symbols
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "GY-521:GY-521"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "ACC"
				(at -9.652 11.938 0)
			)
			(property "Value" "GY-521"
				(at 4.572 -11.938 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "MF" "GODREAM FORDREAM CO., LIMITED"
				(at 0 0 0)
			)
			(property "Description_1" "Accéléromètre à trois axes, gyroscope, breakout"
				(at 0 0 0)
			)
			(property "Package" "Package"
				(at 0 0 0)
			)
			(property "Price" "None"
				(at 0 0 0)
			)
			(property "SnapEDA_Link" "https://www.snapeda.com/parts/GY-521/GODREAM+FORDREAM+CO.%252C+LIMITED/view-part/?ref=snap"
				(at 0 0 0)
			)
			(property "MP" "GY-521"
				(at 0 0 0)
			)
			(property "Availability" "Not in stock"
				(at 0 0 0)
			)
			(property "Check_prices" "https://www.snapeda.com/parts/GY-521/GODREAM+FORDREAM+CO.%252C+LIMITED/view-part/?ref=eda"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "GY-521"
				(at 0 0 0)
			)
			(symbol "GY-521_0_0"
				(polyline
					(pts
						(xy -11.43 -9.43) (xy -11.43 9.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -9.43 11.43) (xy 4.35 11.43)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start -11.43 9.43)
					(mid -10.8442 10.8442)
					(end -9.43 11.43)
					(fill
						(type none)
					)
				)
				(arc
					(start -9.43 -11.43)
					(mid -10.8442 -10.8442)
					(end -11.43 -9.43)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -3.175) (xy -3.175 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -3.175) (xy -1.27 -3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 5.08) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -3.175 -3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 0)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 3.81) (xy 0 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.27) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.35 11.43)
					(mid 5.7642 10.8442)
					(end 6.35 9.43)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.35 -9.43)
					(mid 5.7642 -10.8442)
					(end 4.35 -11.43)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.35 -11.43) (xy -9.43 -11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 3.81 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 9.43) (xy 6.35 -9.43)
					)
					(fill
						(type none)
					)
				)
				(text "MPU"
					(at 0 -10.16 0)
				)
				(pin power_in line
					(at -16.51 8.89 0)
					(length 5.08)
					(name "VCC")
					(number "VCC")
				)
				(pin power_in line
					(at -16.51 6.35 0)
					(length 5.08)
					(name "GND")
					(number "GND")
				)
				(pin bidirectional line
					(at -16.51 3.81 0)
					(length 5.08)
					(name "SCL")
					(number "SCL")
				)
				(pin bidirectional line
					(at -16.51 1.27 0)
					(length 5.08)
					(name "SDA")
					(number "SDA")
				)
				(pin bidirectional line
					(at -16.51 -1.27 0)
					(length 5.08)
					(name "XDA")
					(number "XDA")
				)
				(pin bidirectional line
					(at -16.51 -3.81 0)
					(length 5.08)
					(name "XCL")
					(number "XCL")
				)
				(pin bidirectional line
					(at -16.51 -6.35 0)
					(length 5.08)
					(name "AD0")
					(number "AD0")
				)
				(pin bidirectional line
					(at -16.51 -8.89 0)
					(length 5.08)
					(name "INT")
					(number "INT")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_Module:Arduino_UNO_R3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at -10.16 23.495 0)
			)
			(property "Value" "Arduino_UNO_R3"
				(at 5.08 -26.67 0)
			)
			(property "Footprint" "Module:Arduino_UNO_R3"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
				(at 0 0 0)
			)
			(property "Description" "Arduino UNO Microcontroller Module, release 3"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino*UNO*R3*"
				(at 0 0 0)
			)
			(symbol "Arduino_UNO_R3_0_1"
				(rectangle
					(start -10.16 22.86)
					(end 10.16 -25.4)
					(fill
						(type background)
					)
				)
			)
			(symbol "Arduino_UNO_R3_1_1"
				(pin bidirectional line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "D0/RX")
					(number "15")
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D1/TX")
					(number "16")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D2")
					(number "17")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D3")
					(number "18")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D4")
					(number "19")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D5")
					(number "20")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D6")
					(number "21")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D7")
					(number "22")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D8")
					(number "23")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D9")
					(number "24")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D10")
					(number "25")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D11")
					(number "26")
				)
				(pin bidirectional line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "D12")
					(number "27")
				)
				(pin bidirectional line
					(at -12.7 -17.78 0)
					(length 2.54)
					(name "D13")
					(number "28")
				)
				(pin no_connect line
					(at -10.16 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin power_in line
					(at -2.54 25.4 270)
					(length 2.54)
					(name "VIN")
					(number "8")
				)
				(pin power_in line
					(at -2.54 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "29")
				)
				(pin power_in line
					(at 0 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin power_out line
					(at 2.54 25.4 270)
					(length 2.54)
					(name "3V3")
					(number "4")
				)
				(pin power_in line
					(at 2.54 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin power_out line
					(at 5.08 25.4 270)
					(length 2.54)
					(name "+5V")
					(number "5")
				)
				(pin input line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin output line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "IOREF")
					(number "2")
				)
				(pin input line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "AREF")
					(number "30")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "A0")
					(number "9")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A1")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A2")
					(number "11")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "A3")
					(number "12")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "SDA/A4")
					(number "13")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "SCL/A5")
					(number "14")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "SDA/A4")
					(number "31")
				)
				(pin bidirectional line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "SCL/A5")
					(number "32")
				)
			)
			(embedded_fonts no)
		)
		(symbol "lcd16x2_i2c:LCD16X2_I2C"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "DS"
				(at -20.32 10.16 0)
			)
			(property "Value" "LCD16X2_I2C"
				(at 17.78 10.16 0)
			)
			(property "Footprint" "WC1602A"
				(at 0 -1.27 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "MODULE_LCD-16X2"
				(at 0 0 0)
			)
			(symbol "LCD16X2_I2C_0_0"
				(text "16x2"
					(at 0 2.54 0)
				)
			)
			(symbol "LCD16X2_I2C_0_1"
				(rectangle
					(start -21.59 8.89)
					(end 21.59 -8.89)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -19.05 6.35)
					(end 19.05 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "LCD16X2_I2C_1_1"
				(pin power_in line
					(at -19.05 -12.7 90)
					(length 3.81)
					(name "VSS")
					(number "1")
				)
				(pin power_in line
					(at -16.51 -12.7 90)
					(length 3.81)
					(name "VDD")
					(number "2")
				)
				(pin bidirectional line
					(at -7.62 -12.7 90)
					(length 3.81)
					(name "SDA")
					(number "3")
				)
				(pin input clock
					(at -5.08 -12.7 90)
					(length 3.81)
					(name "SCL")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:VCC"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "VCC"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"VCC\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "VCC_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "GY-521(MPU6050)"
		(exclude_from_sim no)
		(at 183.896 106.68 0)
	)
	(text "Arduino UNO"
		(exclude_from_sim no)
		(at 87.376 45.72 0)
	)
	(text "Ecran LCD 16x2 I2C"
		(exclude_from_sim no)
		(at 175.006 36.83 0)
	)
	(junction
		(at 165.1 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 135.89)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 186.69 133.35)
	)
	(no_connect
		(at 90.17 81.28)
	)
	(no_connect
		(at 115.57 93.98)
	)
	(no_connect
		(at 115.57 91.44)
	)
	(no_connect
		(at 115.57 88.9)
	)
	(no_connect
		(at 90.17 78.74)
	)
	(no_connect
		(at 90.17 101.6)
	)
	(no_connect
		(at 90.17 71.12)
	)
	(no_connect
		(at 115.57 78.74)
	)
	(no_connect
		(at 90.17 86.36)
	)
	(no_connect
		(at 100.33 58.42)
	)
	(no_connect
		(at 90.17 99.06)
	)
	(no_connect
		(at 90.17 91.44)
	)
	(no_connect
		(at 90.17 76.2)
	)
	(no_connect
		(at 115.57 68.58)
	)
	(no_connect
		(at 90.17 96.52)
	)
	(no_connect
		(at 90.17 73.66)
	)
	(no_connect
		(at 115.57 96.52)
	)
	(no_connect
		(at 186.69 130.81)
	)
	(no_connect
		(at 90.17 93.98)
	)
	(no_connect
		(at 105.41 58.42)
	)
	(no_connect
		(at 186.69 138.43)
	)
	(no_connect
		(at 115.57 86.36)
	)
	(no_connect
		(at 90.17 68.58)
	)
	(no_connect
		(at 90.17 83.82)
	)
	(no_connect
		(at 115.57 83.82)
	)
	(no_connect
		(at 90.17 88.9)
	)
	(no_connect
		(at 115.57 73.66)
	)
	(wire
		(pts
			(xy 165.1 50.8) (xy 172.72 50.8)
		)
	)
	(wire
		(pts
			(xy 172.72 58.42) (xy 172.72 59.69)
		)
	)
	(wire
		(pts
			(xy 181.61 125.73) (xy 186.69 125.73)
		)
	)
	(wire
		(pts
			(xy 165.1 48.26) (xy 165.1 50.8)
		)
	)
	(wire
		(pts
			(xy 177.8 135.89) (xy 186.69 135.89)
		)
	)
	(wire
		(pts
			(xy 115.57 104.14) (xy 120.65 104.14)
		)
	)
	(wire
		(pts
			(xy 177.8 115.57) (xy 177.8 120.65)
		)
	)
	(wire
		(pts
			(xy 181.61 128.27) (xy 186.69 128.27)
		)
	)
	(wire
		(pts
			(xy 100.33 111.76) (xy 100.33 115.57)
		)
	)
	(wire
		(pts
			(xy 177.8 120.65) (xy 186.69 120.65)
		)
	)
	(wire
		(pts
			(xy 105.41 115.57) (xy 102.87 115.57)
		)
	)
	(wire
		(pts
			(xy 165.1 53.34) (xy 165.1 50.8)
		)
	)
	(wire
		(pts
			(xy 102.87 115.57) (xy 102.87 119.38)
		)
	)
	(wire
		(pts
			(xy 185.42 48.26) (xy 182.88 48.26)
		)
	)
	(wire
		(pts
			(xy 172.72 50.8) (xy 185.42 50.8)
		)
	)
	(wire
		(pts
			(xy 105.41 111.76) (xy 105.41 115.57)
		)
	)
	(wire
		(pts
			(xy 177.8 135.89) (xy 177.8 140.97)
		)
	)
	(wire
		(pts
			(xy 177.8 123.19) (xy 177.8 135.89)
		)
	)
	(wire
		(pts
			(xy 172.72 59.69) (xy 185.42 59.69)
		)
	)
	(wire
		(pts
			(xy 100.33 115.57) (xy 102.87 115.57)
		)
	)
	(wire
		(pts
			(xy 107.95 55.88) (xy 107.95 58.42)
		)
	)
	(wire
		(pts
			(xy 165.1 62.23) (xy 185.42 62.23)
		)
	)
	(wire
		(pts
			(xy 186.69 123.19) (xy 177.8 123.19)
		)
	)
	(wire
		(pts
			(xy 115.57 101.6) (xy 120.65 101.6)
		)
	)
	(wire
		(pts
			(xy 102.87 115.57) (xy 102.87 111.76)
		)
	)
	(wire
		(pts
			(xy 182.88 48.26) (xy 182.88 53.34)
		)
	)
	(wire
		(pts
			(xy 165.1 60.96) (xy 165.1 62.23)
		)
	)
	(label "SDA"
		(at 120.65 101.6 0)
	)
	(label "SCL"
		(at 120.65 104.14 0)
	)
	(label "SDA"
		(at 181.61 128.27 0)
	)
	(label "SCL"
		(at 181.61 125.73 0)
	)
	(rule_area
		(polyline
			(pts
				(xy 80.01 46.99) (xy 132.08 46.99) (xy 134.62 49.53) (xy 134.62 127) (xy 132.08 129.54) (xy 80.01 129.54)
				(xy 77.47 127) (xy 77.47 49.53)
			)
			(fill
				(type none)
			)
		)
	)
	(rule_area
		(polyline
			(pts
				(xy 172.72 109.22) (xy 173.99 107.95) (xy 217.17 107.95) (xy 218.44 109.22) (xy 218.44 147.32) (xy 217.17 148.59)
				(xy 173.99 148.59) (xy 172.72 147.32)
			)
			(fill
				(type none)
			)
		)
	)
	(rule_area
		(polyline
			(pts
				(xy 161.29 40.64) (xy 163.83 38.1) (xy 220.98 38.1) (xy 223.52 40.64) (xy 223.52 91.44) (xy 222.25 92.71)
				(xy 163.83 92.71) (xy 161.29 90.17)
			)
			(fill
				(type none)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 182.88 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 182.88 59.69 0)
		)
		(property "Value" "GND"
			(at 182.88 58.42 0)
		)
		(property "Footprint" ""
			(at 182.88 53.34 0)
		)
		(property "Datasheet" ""
			(at 182.88 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 182.88 53.34 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 177.8 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 177.8 119.38 0)
		)
		(property "Value" "VCC"
			(at 177.8 110.49 0)
		)
		(property "Footprint" ""
			(at 177.8 115.57 0)
		)
		(property "Datasheet" ""
			(at 177.8 115.57 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 177.8 115.57 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 165.1 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 167.64 55.8799 0)
		)
		(property "Value" "R"
			(at 167.64 58.4199 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal"
			(at 163.322 57.15 90)
		)
		(property "Datasheet" "~"
			(at 165.1 57.15 0)
		)
		(property "Description" "Resistor"
			(at 165.1 57.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "GY-521:GY-521")
		(at 203.2 129.54 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "ACC1"
			(at 210.82 128.2699 0)
		)
		(property "Value" "GY-521"
			(at 210.82 130.8099 0)
		)
		(property "Footprint" "GY-521:GY-521"
			(at 203.2 129.54 0)
		)
		(property "Datasheet" ""
			(at 203.2 129.54 0)
		)
		(property "Description" ""
			(at 203.2 129.54 0)
		)
		(property "MF" "GODREAM FORDREAM CO., LIMITED"
			(at 203.2 129.54 0)
		)
		(property "Description_1" "Accéléromètre à trois axes, gyroscope, breakout"
			(at 203.2 129.54 0)
		)
		(property "Package" "Package"
			(at 203.2 129.54 0)
		)
		(property "Price" "None"
			(at 203.2 129.54 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/GY-521/GODREAM+FORDREAM+CO.%252C+LIMITED/view-part/?ref=snap"
			(at 203.2 129.54 0)
		)
		(property "MP" "GY-521"
			(at 203.2 129.54 0)
		)
		(property "Availability" "Not in stock"
			(at 203.2 129.54 0)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/GY-521/GODREAM+FORDREAM+CO.%252C+LIMITED/view-part/?ref=eda"
			(at 203.2 129.54 0)
		)
		(pin "SDA")
		(pin "INT")
		(pin "VCC")
		(pin "GND")
		(pin "SCL")
		(pin "XDA")
		(pin "AD0")
		(pin "XCL")
		(instances
			(project ""
				(path
					(reference "ACC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 102.87 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 102.87 125.73 0)
		)
		(property "Value" "GND"
			(at 102.87 124.46 0)
		)
		(property "Footprint" ""
			(at 102.87 119.38 0)
		)
		(property "Datasheet" ""
			(at 102.87 119.38 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 102.87 119.38 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "lcd16x2_i2c:LCD16X2_I2C")
		(at 198.12 67.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "DS1"
			(at 208.28 66.0399 90)
		)
		(property "Value" "LCD16X2_I2C"
			(at 208.28 68.5799 90)
		)
		(property "Footprint" "LCD-16X2:MODULE_LCD-16X2"
			(at 196.85 67.31 0)
		)
		(property "Datasheet" ""
			(at 198.12 67.31 0)
		)
		(property "Description" ""
			(at 198.12 67.31 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "DS1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 165.1 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 165.1 52.07 0)
		)
		(property "Value" "VCC"
			(at 165.1 43.18 0)
		)
		(property "Footprint" ""
			(at 165.1 48.26 0)
		)
		(property "Datasheet" ""
			(at 165.1 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 165.1 48.26 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 177.8 140.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 177.8 147.32 0)
		)
		(property "Value" "GND"
			(at 177.8 146.05 0)
		)
		(property "Footprint" ""
			(at 177.8 140.97 0)
		)
		(property "Datasheet" ""
			(at 177.8 140.97 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 177.8 140.97 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Module:Arduino_UNO_R3")
		(at 102.87 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "A1"
			(at 110.0933 55.88 0)
		)
		(property "Value" "Arduino_UNO_R3"
			(at 110.0933 58.42 0)
		)
		(property "Footprint" "Module:Arduino_UNO_R3"
			(at 102.87 83.82 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
			(at 102.87 83.82 0)
		)
		(property "Description" "Arduino UNO Microcontroller Module, release 3"
			(at 102.87 83.82 0)
		)
		(pin "6")
		(pin "20")
		(pin "11")
		(pin "14")
		(pin "18")
		(pin "19")
		(pin "9")
		(pin "15")
		(pin "31")
		(pin "23")
		(pin "1")
		(pin "17")
		(pin "4")
		(pin "22")
		(pin "8")
		(pin "3")
		(pin "26")
		(pin "7")
		(pin "10")
		(pin "13")
		(pin "25")
		(pin "30")
		(pin "32")
		(pin "29")
		(pin "24")
		(pin "5")
		(pin "2")
		(pin "16")
		(pin "21")
		(pin "28")
		(pin "12")
		(pin "27")
		(instances
			(project ""
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 107.95 55.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 107.95 59.69 0)
		)
		(property "Value" "VCC"
			(at 107.95 50.8 0)
		)
		(property "Footprint" ""
			(at 107.95 55.88 0)
		)
		(property "Datasheet" ""
			(at 107.95 55.88 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 107.95 55.88 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 172.72 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 175.26 53.3399 0)
		)
		(property "Value" "R"
			(at 175.26 55.8799 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal"
			(at 170.942 54.61 90)
		)
		(property "Datasheet" "~"
			(at 172.72 54.61 0)
		)
		(property "Description" "Resistor"
			(at 172.72 54.61 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
